Gain can be changed in steps of 0.046dB to a maximum of 24dB. Min is -2.81dB.

Register is 820h and has three states (Manual/Abs, Manual, Auto).

ABS\_VAL\_GAIN register =

Gamma ranges from 0.5 to 4.

Register is 818h (0x818). To obtain a linear response, set gamma to 1 or turn it off. Same format as brightness (800h, page 105).

Sharpness ranges from 0 to 4095. For values less than 1000, there is blurring. For values greater than 1000, there is sharpening.

Register is 808h. Format is same as brightness (800h, page 105).